SERVICE BROWSER setting items

| Print out this category

SERVICE BROWSER setting items

Item | Description
BRWS-ACT ([Lv.1] COPIER > Function > INSTALL) | Execution of activation/ inactivation of service browsing Browsing info is sent to UGW when OFF (BRWS-ACT=0) is changed to ACTIVE. Setting result is displayed as "OK!" or "NG!".
BRWS-STS ([Lv.1] COPIER > Display > USER) | Display of Service Browser use status 0: OFF / 1: Active / 2: Suspend The status is changed from 0 to 1, from 1 to 2, and from 2 to 1 by execution of BRWS-ACT. Default : 0 (OFF)

NOTE:
Generally, once service browsing is enabled, it cannot be disabled again.
To disable service browsing, clear SRAM.