﻿Removing the Developing Assembly

| Print out this category

﻿Image Formation System
Removing the Developing Assembly
<Procedure>
1) Open the right cover.
2) Open the front cover.
3) Remove the waste toner container. (Reference)
4) Remove the drum unit. (Reference)
5) Remove the toner supply cover. (Reference)
6) Remove the developing assembly
1 connector
CAUTION:
When installing the developing assembly, insert the developing assembly while its guide engages with the rail of the host machine.