Preparation for Relocating the Machine

| Print out this category

Preparation for Relocating the Machine
When moving the machine using stairs (including steps) or transporting the machine to a different place using a truck, go through the steps described below.
CAUTION:
When lifting the machine with a double-cassette pedestal, be sure to remove the double-cassette pedestal in advance.
If the machine is lifted with the double-cassette pedestal installed, they may separate from each other and consequently the machine can damage.
NOTE:
When dividing the reader part and the printer part, refer to the follwing procedure.
"Removing the Reader Assembly."