Main Controller PCB 1

| Print out this category

Main Controller PCB 1
<Procedure of parts replacement>
Main Controller PCB 1
<Procedure of adjustment>
Service part:
Setting unit: Main Controller PCB 1 + Controller Box Frame + Cooling Fan
Parts number differs on a model basis (speed basis).
In order to secure the accuracy of connector connection when slotting in, this service part is provided with the PCB being installed to the frame.
1) Transferring the parts from old PCB to new PCB
DDR2-SDRAM (2 pc.)
Flash PCB
TPM PCB
NOTE:
Resetting/registering the data is not necessary after Main Controller PCB 1 is replaced.