﻿Updating Downloaded Firmware (Applying Firmware)

| Print out this category

﻿Updating Downloaded Firmware (Applying Firmware)
This section describes how to update the downloaded firmware.
1. Start [Service Mode] at Level 1.
1). Press [Setting/Registration (User mode)] button on the control panel.
2). Press [2] and [8] buttons at a time on the control panel.
3). Press [Setting/Registration (User mode)] button on the control panel.
4). [Service Mode] screen is shown.
2. Press [Updater] button.
3. Press [Update Firmware] button.
4. Press [Apply Firmware] button.
5. Confirm the downloaded firmware and press [Yes] button.
6. The firmware is applied to the device. The device is automatically restarted when the firmware is successfully applied.
7. When the device is restarted, confirm the version of the firmware.
1). Press [Check Counter Key] button on the control panel.
2). Press [Check Device Configuration] button.
3). Confirm if the updated firmware version corresponds to [Controller Version].
Now the firmware is successfully updated in the method.