Mechanism

| Print out this category

Mechanism
MEAP platform judges whether MEAP applications can be operated on it using on the 2 information below:
Device Specification ID
MEAP Specifications
Device Specification ID shows information such as the original functions of MFP (including print, scan, and copy), and one that differs by model such as maximum copy number, thus each model has a different ID. (It is easy to determine the IDs for this reason.) MEAP application declares 1 or more Device Specification ID required for its execution. Declaration of multiple Device Specification IDs means that the application is operable in all the models declared. Upon installation of MEAP application in (using) SMS or MEAP Enterprise Service Manager, matching of Device Specification ID is executed on the side of MEAP platform machine. The machine which doesn't support the ID declared by the application rejects installation of such an application.
Meanwhile, MEAP Specifications shows other information than defined by Device Specification ID above, including network and security. Thus each model does not always have the same version.
MEAP application declares 1 or more MEAP Specifications required for its execution.
Declaration of multiple Device Specification IDs means that the application is operable in all the environments declared. Upon installation of MEAP application in SMS or MEAP Enterprise Service Manager, matching of MEAP Specifications is executed on the side of MEAP platform machine. The machine which doesn't support the version declared by the application rejects installation of such an application.
MEAP Specifications for each model

Product Name | Initial MEAP SpecVer | Remarks

iR-ADV C5051
iR-ADV C5045
iR-ADV C5035
iR-ADV C5030

5, 6, 7, 9, 10, 11, 13, 14, 15, 17, 18, 19, 25, 26, 27, 29, 30, 31, 32, 33, 34, 35, 36, 37, 38, 39, 40, 41, 42, 44, 45

Ver.37.xx or later
5, 6, 7, 9, 10, 11, 13, 14, 15, 17, 18, 19, 25, 26, 27, 29, 30, 31, 32, 33, 34, 35, 36, 37, 38, 39, 40, 41, 42, 44, 45, 46
Ver.38.xx or later
5, 6, 7, 9, 10, 11, 13, 14, 15, 17, 18, 19, 25, 26, 27, 29, 30, 31, 32, 33, 34, 35, 36, 37, 38, 39, 40, 41, 42, 44, 45, 46, 49
Ver.50.xx or later
5,6,7,9,10,11,13,14,15,17,18,19,25,26,27,29,30,31,32,33,34,35,36,37,38,39,40,41,42,44,45,46,47,49,50,51,52,53,54,55,56,57,58,59

iR-ADV C9075
iR-ADV C9070
iR-ADV C9065
iR-ADV C9060
iR-ADV C7065
iR-ADV C7055

5, 6, 7, 9, 10, 11, 13, 14, 15, 17, 18, 19, 25, 26, 27, 29, 30, 31, 32, 33, 34, 35, 36, 37, 38, 39, 40, 41, 42, 44, 45

Ver.37.xx or later
5, 6, 7, 9, 10, 11, 13, 14, 15, 17, 18, 19, 25, 26, 27, 29, 30, 31, 32, 33, 34, 35, 36, 37, 38, 39, 40, 41, 42, 44, 45, 46
Ver.38.xx or later
5, 6, 7, 9, 10, 11, 13, 14, 15, 17, 18, 19, 25, 26, 27, 29, 30, 31, 32, 33, 34, 35, 36, 37, 38, 39, 40, 41, 42, 44, 45, 46, 49
Ver.50.xx or later
5, 6, 7, 9, 10, 11, 13, 14, 15, 17, 18, 19, 25, 26, 27, 29, 30, 31, 32, 33, 34, 35, 36, 37, 38, 39, 40, 41, 42, 44, 45, 46, 47, 49, 50, 51, 52, 53, 54, 55, 56, 57, 58, 59

iR-ADV 6075 iR-ADV 6065 iR-ADV 6055 | 5, 6, 7, 9, 10, 11, 13, 14, 15, 17, 18, 19, 25, 26, 27, 29, 30, 31, 32, 33, 34, 35, 36, 37, 38, 39, 40, 41, 44, 45, 46, 49 | Ver.20.xx or later 5, 6, 7, 9, 10, 11, 13, 14, 15, 17, 18, 19, 25, 26, 27, 29, 30, 31, 32, 33, 34, 35, 36, 37, 38, 39, 40, 41, 44, 45, 46, 49, 50, 51, 52, 53, 54, 55, 56, 57, 58, 59
iR-ADV 8105 PRO iR-ADV 8095 PRO iR-ADV 8085 PRO | 5, 6, 7, 9, 10, 11, 13, 14, 15, 17, 18, 19, 25, 26, 27, 29, 30, 31, 32, 33, 34, 35, 36, 37, 38, 39, 40, 41, 44, 45, 46, 49 | Ver.20.xx or later 5, 6, 7, 9, 10, 11, 13, 14, 15, 17, 18, 19, 25, 26, 27, 29, 30, 31, 32, 33, 34, 35, 36, 37, 38, 39, 40 , 41, 44, 45, 46, 49, 50, 51, 52, 53, 54, 55, 56, 57, 58, 59
iR-ADV C2030 iR-ADV C2025 iR-ADV C2020 | 5, 6, 7, 9, 10, 11, 13, 14, 15, 17, 18, 19, 25, 26, 27, 29, 30, 31, 32, 33, 34, 35, 36, 37, 38, 39, 40, 41, 42, 44, 45, 46, 47, 48, 49 | Ver.10.xx or later 5, 6, 7, 9, 10, 11, 13, 14, 15, 17, 18, 19,25, 26, 27, 29, 30, 31, 32, 33, 34, 35, 36, 37, 38, 39, 40, 41, 42, 44, 45, 46, 47, 48, 49, 53
iR-ADV 4051 iR-ADV 4045 iR-ADV 4035 iR-ADV 4025 | 5, 6, 7, 9, 10, 11, 13, 14, 15, 17, 18, 19, 25, 26, 27, 29, 30, 31, 32, 33, 34, 35, 36, 37, 38, 39, 40, 41, 42, 44, 45, 46, 47, 49, 50, 51, 52, 53, 54, 55, 56, 57, 58, 59 |

MEAP Specifications List

Ver | Description
1 | MEAP basic function
2 | MEAP Spec Version 1 function and SSL/TSL + Proxy
5 | MEAP Spec Version 1 function and CPCA V2 + ERS (Error Recovery Service) + New SSL/TSL
6 | Reserved
7 | MEAP Spec Version 5 function and Compact PDF + OCR PDF (Text Searchable) + USB Host (Buffering of Interrupt Transfer)
9 | Reserved
10 | MEAP Spec Version 5 function and USB-Host (Exception + Clear Feature + Set Feature+ Hot Plug) + WINS address acquisition using MIB Agent + Timer Service + SSL client authentication
11 | MEAP Spec Version 5 function and AMS
13 | MEAP Spec Version 5 function and J2ME1.1 Support + Encrypted PDF + Trace and smooth PDF + CTK2.0
14 | Device signature PDF
15 | IMI + ERS (API addition for IMI) , IPv6, Extended encryption function (AES/RC4)
17 | Acquiring images of JBIG format
18 | Parsing XML documents (XML parser)
19 | Enhancement of IMI function (IMI Version1.2 series)
21 | Reserved
25 | API to access the HID/Mass Storage class devices.
26 | MEAP driver preference function
27 | Symbols that can be used with MibAgent added. (symbols for IPv6 address acquisition)
29 | IMI API added (IMI version 1.2.1 enabled)
30 | Extended address book function. (e-mail/group/i-FAX/file)
31 | Integrated ERS function
32 | Extended Imaging function (function to generate PDF/OOXML (PowerPoint) with visible signature)
33 | Extended function for imageRUNNER / iR ADVANCE series (API for address book/ CTK/TopMenu)
34 | Extended IMI Box function (v1.3.0)
35 | Extended SIS function (function to check the network cable status, function to check PS print server unit status)
36 | Reserved
37 | CLS (Contextual Login Service) Supporting API Added
38 | imageRUNNER / iR ADVANCE Series administrative privileges supported
39 | MEAP Specifications added according to Jcrypto API Specification Change
40 | ImagingAPI (Creation API of Visible Signature PDF) added
41 | Reserved
42 | Reserved
44 | imageRUNNER / iR ADVANCE Series Remote Address Book Supported, RemoteFAX Supported.
45 | Addition of API that allows acquisition of the HID installation status
46 | Multilingualization of the USB keyboard of the System Driver
47 | Addition of API which executes a print order from the MEAP application of the IMI encryption PDF document
48 | ID expressing the scan function for iR-ADV C2030/C2025/C2020 series
49 | Reserved
50 | SecurityOptionalPackage
51 | IMI function expansion of iR-ADV C5051 series (Ver.50.xx or later) or later
52 | (iR-ADV C5051 series (Ver.50.xx or later)) Addition of registered API to enable SSL communication setting (On/Off) for each URL
53 | Disclosure of registration/deletion function to/from Quick Menu
54 | Function to notify an event to the application at recovery from the sleep mode.
55 | System account release function
56 | MEAP User Preference Service
57 | MEAP Application Configuration Service
58 | MEAP Application Log Service
59 | Reserved