Downloading/Writing System Software (Automatic)

| Print out this category

Downloading/Writing System Software (Automatic)
[1]: Upgrade (Auto)
The version is compared between the host machine/option and the system software in the USB memory storage device to download only the system software with newer version in the USB memory storage device to the temporary storage area of the HDD.
In safe mode, only the following system software can retrieve the version information (the version is compared).
SYSTEM, LANGUAGE, RUI, MERAPCONT, SDICT
As for system software of the host machine whose version information cannot be obtained, the software for RCON is not downloaded, but other software are downloaded.
For the system software of the option that is not connected, it is handled as follows:
<In the case of startup in normal mode (Recommended)>
For the option that is not connected, the system software is not to be downloaded.
<In the case of startup in safe mode>
The system software of the options which are not connected are not downloaded.
After downloading is complete, this machine is automatically restarted to write the downloaded system software to the HDD system area/flash ROM.
Operation procedure
1) Enter download mode.
2) Connect the USB memory storage device to the USB port.
3) Press the key on the Control Panel.
[1] -> [0]: To execute downloading/Any key other than [0] key: To return to the menu screen.
During downloading, download status is displayed on the Control Panel.
Once downloading is complete, this machine is automatically restarted to start writing to the HDD system area/flash ROM.
The screen shows the countdown once writing process is properly complete.
Once the countdown shows 0, this machine is automatically restarted.
4) When the main menu is displayed, press the removal key at the lower right on the touch panel and select removal of the memory media, and then remove the USB memory storage device.
CAUTION:
After HDD formatting and downloading, this machine takes a long time (for writing the software).
This machine, in some cases, stays in standby screen up to 10 min during writing. At this time, do not turn off the main power switch.