OPTION

| Print out this category

﻿BOARD
OPTION

BOARD>OPTION
MENU-1 | Hide/dis of printer setting menu level 1
Lv.2 | Details | To set whether to display or hide the level 1 of printer setting menu.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Hide, 1: Display
Default value | 0
MENU-2 | Hide/dis of printer setting menu level 2
Lv.2 | Details | To set whether to display or hide the level 2 of printer setting menu.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Hide, 1: Display
Default value | 0
MENU-3 | Hide/dis of printer setting menu level 3
Lv.2 | Details | To set whether to display or hide the level 3 of printer setting menu.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Hide, 1: Display
Default value | 0
MENU-4 | Hide/dis of printer setting menu level 4
Lv.2 | Details | To set whether to display or hide the level 4 of printer setting menu.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Hide, 1: Display
Default value | 0
FONTDL | ON/OFF of font setting screen display
Lv.1 | Details | To set whether to display the service-purposed setting screen of fonts which are listed using PS Kanji Font Downloader.
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Hide, 1: Display
Default value | 0