Counter control

| Print out this category

Counter control
Count-up timing differs according to the following.
Print mode (1-sided page, 2nd side of 2-sided page, 1st side of 2-sided page)
Delivery position (Finisher).

Target of delivery | Print mode
Single-sided/Doublesided (2nd side) | Double-sided (1st side)
Count-up timing
Host machine | 1st delivery tray | No.1 delivery sensor (S12) | Duplex feed sensor (S7)
2nd delivery tray | No. 2 delivery sensor (S42)
Inner finisher | Inner finisher inlet sensor (S1)
Staple Finisher / Booklet Finisher | Tray A (Upper Tray) | Reference Sensor: Feed Path Sensor (S102)
Tray B (Lower Tray)
Saddle area | Reference Sensor: Saddle inlet sensor (S201)

Default counters for each country (model) are listed below.

Target | Display number of each counter (in service mode) / item | Country Code
Counter 1 | Counter 2 | Counter 3 | Counter 4 | Counter 5 | Counter 6 | Counter 7 | Counter 8
JP model Type1 (Conventional method) | Total 1 | Total (Black 1) | Copy (Full Color + Single Color/1) | Total A (Full Color + Single Color 1) | *1 | *1 | *1 | *1 | JP
101 | 108 | 232 | 149 | 000 | 000 | 000 | 000
JP model Type 2 (New method) | Total 2 | Copy (Full Color + Single Color/2) | Total A (Full Color + Single Color/2) | Copy (Black 2) | Total A (Black 2) | *1 | *1 | *1 | JP
102 | 231 | 148 | 222 | 133 | 000 | 000 | 000
JP model Type 3 (New method) | Total 1 | Total (Black 1) | Copy (Full Color + Single Color/1) | Total A (Full Color + Single Color 1) | Total (Single Color 1) | *1 | *1 | *1 | JP
101 | 108 | 232 | 149 | 118 | 0 | 000 | 000
JP model Type4 (New method) | Total 1 | Total (Full Color + Single Color/Small) | Total (Full Color + Single Color/Large) | Total (Black/Small) | Total (Black/Large) | Scan (Total 1) | *1 | *1 | JP
101 | 123 | 122 | 113 | 112 | 501 | 000 | 000
JP model Type5 (New method) | Total 1 | Total (Full Color + Single Color/Small) | Total (Full Color + Single Color/Large) | Total (Black/Small) | Total (Black/Large) | Total (Single Color/Small) | Total (Single Color/Large) | Scan (Total 1) | JP
101 | 123 | 122 | 113 | 112 | 111 | 110 | 501
Taiwan model | Total 1 | Total (Black 1) | Copy + Print (Full Color/Large) | Copy + Print (Full Color/Small) | Total (Single Color 1) | *1 | *1 | *1 | TW
101 | 108 | 401 | 402 | 118 | 000 | 000 | 000
UL model Type1 (Conventional method) | Total 1 | Total (Black 1) | Copy (Full Color + Single Color/Large) | Copy (Full Color + Single Color/Small) | Print (Full Color + Single Color/Large) | Print (Full Color + Single Color/Small) | *1 | *1 | US
101 | 108 | 229 | 230 | 321 | 322 | 000 | 000
UL model Type 2 (New method) | Total 2 | Total (Black 2) | Copy (Full Color + Single Color/Large) | Copy (Full Color + Single Color/Small) | Print (Full Color + Single Color/Large) | Print (Full Color + Single Color/Small) | *1 | *1 | US
102 | 109 | 229 | 230 | 321 | 322 | 000 | 000
General model | Total 1 | Total (Black 1) | Copy + Print (Full Color/Large) | Copy + Print (Full Color/Small) | Total (Single Color 1) | Total 1 (Duplex) | *1 | *1 | SG/KO/CN
101 | 108 | 401 | 402 | 118 | 114 | 000 | 000
UK model Type1 (Conventional method) | Total (Black/Large) | Total (Black/Small) | Total (Full Color + Single Color/Large) | Total (Full Color + Single Color/Small) | Scan (Total 1) | Print (Total 1) | *1 | *1 | GB
112 | 113 | 122 | 123 | 501 | 301 | 000 | 000
240V UK model Type 2 (New method) | Total 1 | *1 | *1 | *1 | *1 | *1 | *1 | *1 | GB
101 | 000 | 000 | 000 | 000 | 000 | 000 | 000
CA model | Total 1 | Total (Black 1) | Copy (Full Color + Single Color/Large) | Copy (Full Color + Single Color/Small) | Print (Full Color + Single Color/Large) | Print (Full Color + Single Color/Small) | *1 | *1 | AU
101 | 108 | 229 | 230 | 321 | 322 | 000 | 000
FRN model Type1 (Conventional method) | Total (Black/Large) | Total (Black/Small) | Total (Full Color + Single Color/Large) | Total (Full Color + Single Color/Small) | Scan (Total 1) | Print (Total 1) | *1 | *1 | FR
112 | 113 | 122 | 123 | 501 | 301 | 000 | 000
FRN model Type 2 (New method) | Total 1 | *1 | *1 | *1 | *1 | *1 | *1 | *1 | FR
101 | 000 | 000 | 000 | 000 | 000 | 000 | 000
GER model Type1 (Conventional method) | Total (Black/Large) | Total (Black/Small) | Total (Full Color + Single Color/Large) | Total (Full Color + Single Color/Small) | Scan (Total 1) | Print (Total 1) | *1 | *1 | DE
112 | 113 | 122 | 123 | 501 | 301 | 000 | 000
GER model Type 2 (New method) | Total 1 | *1 | *1 | *1 | *1 | *1 | *1 | *1 | DE
101 | 000 | 000 | 000 | 000 | 000 | 000 | 000

AMS model
Type1
(Conventional method)

Total (Black/Large)

Total (Black/Small)

Total (Full Color + Single Color/Large)

Total (Full Color + Single Color/Small)

Scan (Total 1)

Print (Total 1)

*1

*1

ES/SE/
PT/NO/
DK/FI/
PL/HU/
CZ/SI/
GR/EE/
RU/NL/
SK/RO/
HR/BG/
TR

112 | 113 | 122 | 123 | 501 | 301 | 000 | 000

AMS model
Type 2
(New method)

Total 1

*1

*1

*1

*1

*1

*1

*1

ES/SE/
PT/NO/
DK/FI/
PL/HU/
CZ/SI/
GR/EE/
RU/NL/
SK/RO/
HR/BG/
TR

101 | 000 | 000 | 000 | 000 | 000 | 000 | 000
ITA model Type1 (Conventional method) | Total (Black/Large) | Total (Black/Small) | Total (Full Color + Single Color/Large) | Total (Full Color + Single Color/Small) | Scan (Total 1) | Print (Total 1) | *1 | *1 | IT
112 | 113 | 122 | 123 | 501 | 301 | 0 | 0
ITA model Type 2 (New method) | Total 1 | *1 | *1 | *1 | *1 | *1 | *1 | *1 | IT
101 | 000 | 000 | 000 | 000 | 000 | 000 | 000

<Explanation of the list>
Large: Large size paper (when paper length exceeds 364 mm in paper feed direction)
Small: Small size paper (when paper length is 364 mm or less in paper feed direction)
Total: Copy + Print; 1 count up
2-Sided: 1 count up when auto 2-sided copy
Country code change of CONFIG is executed from COPIER > OPTION > FNC-SW > CONFIG.
Three-digit number in the counter column shows the setting value of the following service mode items.
(Lv.1) COPIER > OPTION > USER > COUNTER 1 to 8
COUNTER2 to 8 can be changed from the service mode (COPIER > OPTION > USER).
*1: Nothing is displayed as default. However, you can change this setting from the service mode.