﻿Communication Test

| Print out this category

﻿Communication Test
This section describes how to check if the communication is normally done to the distribution server and/or the file server.
1. Start [Service Mode] at Level 1.
1). Press [Setting/Registration (User Mode)] button on the control panel.
2). Press [2] and [8] buttons at a time on the control panel.
3). Press [Setting/Registration (User Mode)] button on the control panel.
4). [Service Mode] screen is shown.
NOTE:
CDS and RDS are another servers.
You need the communication test of CDS by all means even if You succeed in a communication test of the RDS.
2. Press [Updater] button.
3. Press [Software Management Settings] button.
4. Press [Test Communication] button.
5. Press [Yes] button.
Obtain the download file information for communication test from the distribution server (to execute the communication test to the distribution server).
Using the download file information for communication test, the contents for test are downloaded from the file server (for the communication test to the file server).
6. Upon the communication test completed, the communication test result screen is shown.
Press [OK] button to exit this operation.