Connection

| Print out this category

Connection
CAUTION:
This machine does not communicate with SST once it recognizes a USB memory storage device; therefore, SST and a USB memory storage device cannot be used at the same time.
Preparation
Item to prepare: a USB memory storage device, which the system software for this machine is stored.
Procedure
1) If a cross cable is connected to this machine, remove the cross cable.
2) Connect the USB memory storage device to the USB port.
3) Switch to the download mode to use.
In the case of normal mode (Recommended)
Select the following in Service Mode: COPIER > FUNCTION > SYSTEM > DOWNLOAD; and then press [OK].
In the case of safe mode (This mode should not be used as general rule. To be used only when normal startup fails, such as a system error, etc.)
While pressing 2 + 8 keys at the same time, turn ON the Main Power Switch.
Once this machine recognizes the USB memory storage device, the following menu is displayed on the Control Panel.
CAUTION:
Depending on the manufacturer or the model, this machine may not recognize the USB memory storage device.
This machine retries the detection of a USB memory storage device for up to 60 seconds after power-ON. The above menu is not displayed if the recognition of a USB memory storage device is failed within the time period.
In such a case, use another USB memory storage device.