﻿Removing the Cassette Pickup Unit 2

| Print out this category

Removing the Cassette Pickup Unit 2
1) Draw out the cassette.
2) Open the right cover.
3) Remove the right cover (lower).(only when the cassette feeding unit is not installed)
4) Remove the rear right cover (lower).(Reference)
5) Remove the front right cover (lower).(Reference)
6) Unload the cable harness from the cable guide.
1 connector
7) Remove the cassette pickup unit 2.
4 screws