Manual Saving by Holding Down the Counter + 1.2.3

| Print out this category

Manual Saving by Holding Down the Counter + 1.2.3
1. Reproduce the error.
2. Hold down the [Counter] button (10 sec. or longer).
3. Press 1 on the numeric keypad.
4. Press 2 on the numeric keypad.
5. Press 3 on the numeric keypad. (UI is locked at this stage) The machine starts generation of the file that was converted from Log data on the HDD into text-based data.
The screen does not change even though you press the OK button on the touch panel of the machine. If the screen changes by pressing the OK button, data transfer has been completed.
Lev1 COPIER > FUNCTION > SYSTEM > DOWNLOAD > OK
[5] Execute [BACKUP].
[1] Execute [Sublog].
When the data is sent to the USB memory device:
The file name is "file name ** + year date time.BIN".
Example:
SUBLOG02_201103290130.BIN
Note:
Date to be added to the file name shows the date that the log was transferred.
Display it by time of local Time.