Periodical Service Operation Item

| Print out this category

Periodical Service Operation Item
♦: Replacement (Periodical replacement) ●: Replaced (consumables) Δ: Cleaned

No. | System | Items | Parts No. | Q'ty | Life | Interval | Counter | Remarks
80,000 sheets | 120,000 sheets | 150,000 sheets | 240,000 sheets | 500,000 sheets | 600,000 sheets
1 | Image formation system | Waste toner container | FM3-9276 | 1 | 80,000 sheets | ● |  |  |  |  |  | DRBL-1 | WST-TNR | Defined by 6% document If service engineer removes the waste toner from the Waste Toner Container, the Waste Toner Container can be reused.
2 | Transfer guide | - | 1 | 120,000 sheets |  | Δ |  |  |  |  | - | - | Wipe with dry cloth.
3 | Transfer roller | FC9-0693 | 1 | 240,000 sheets |  |  |  | ● |  |  | DRBL-1 | TR-ROLL |
4 | Separation static charge eliminator | FM3-9296 | 1 | 240,000 sheets |  |  |  | ● |  |  | DRBL-1 | SP-SC-EL |
5 | Developing assembly | FM4-9730 | 1 | 600,000 sheets: 51/45/35cpm 500,000 sheets: 25cpm |  |  |  |  | ● | ● | DRBL-1 | DV-UNT-K |
6 | Pushing wheel (developing assembly) | - | 1 | 120,000 sheets |  | Δ |  |  |  |  | - | - | Dry wiping
7 | Fixing system | Fixing inlet guide | - | 1 | 120,000 sheets |  | Δ |  |  |  |  | - | - | Wipe with dry cloth. If dirt cannot come off, wipe it with alcohol.
8 | Fixing main unit | FM4-9733 (120V_51cpm) FM4-9734 (230V_51cpm) FM4-9736 (120V_45/35/25cpm) FM4-9737 (230V_45/35/25cpm) | 1 | 240,000 sheets |  |  |  | ● |  |  | DRBL-1 | FX-UNIT |
9 | Pickup feed system | Cassette pickup roller | FB6-3405 FC7-9381 (For CHN) | 2 | 120,000 sheets |  | ● |  |  |  |  | DRBL-1 | C1-PU-RL C2-PU-RL |
10 | Cassette feed roller | FC6-7083 FC7-9502 (For CHN) | 2 | 120,000 sheets |  | ● |  |  |  |  | DRBL-1 | - |
11 | Cassette separation roller | FC6-6661 | 2 | 120,000 sheets |  | ● |  |  |  |  | DRBL-1 | C1-SP-RL C2-SP-RL |
12 | Manual feed pickup roller | FL3-1352 | 1 | 150,000 sheets |  |  | ● |  |  |  | DRBL-1 | M-FD-RL |
13 | Manual feed separation pad | FL3-3469 | 1 | 150,000 sheets |  |  | ● |  |  |  | DRBL-1 | M-SP-PD |
14 | Pre-registration guide (Static charge eliminator) | - | 1 | As needed |  | Δ |  |  |  |  | - | - | Dry wiping with the lint-free paper
15 | External Auxiliary System | Air filter | FC0-3078 | 1 set (2 pcs.) | 240,000 sheets |  |  | ♦ |  |  |  | DRBL-1 | OZ-FIL1 |

CAUTION:
The value is the mean value collected from the results of evaluation. The value may vary depending on the site environment or user habit. The parts number may change because of changes in design.