﻿Stained Leading/Trailing Edge of Paper

| Print out this category

Stained Leading/Trailing Edge of Paper
[Occurrence area]
Transfer front guide
Fixing inlet guide
[Cause]
Transfer front guide: The leading or trailing edge of paper touches the toner stuck to the transfer front upper guide.
Fixing inlet guide: The leading or trailing edge of paper touches the toner stuck to the fixing inlet guide.
[Occurrence condition]
When halftone or solid-black images are printed in succession
[Remedy]
Using lens-cleaning paper or the like, clean the guide stained with toner.