﻿Setting Log Level

| Print out this category

﻿Setting Log Level
This section describes how to set system log levels.
1. Start [Service Mode] at Level 1.
1). Press [Setting/Registration (User Mode)] button on the control panel.
2). Press [2] and [8] buttons at a time on the control panel.
3). Press [Setting/Registration (User Mode)] button on the control panel.
4). [Service Mode] screen is shown.
2. Press [Updater] button.
3. Press [Software Management Settings] button.
4. Press [Settings] button.
5. Select a log level from [Log Level] dropdown list.
[Log Level]:
Select one of 5 levels ranging from [0] to [4].
See the table below for logs output in each level.

Log Level | Log Output
Trace | Information | Important Message | Ordinary Error | System Error
0 | - | - | - | - | Yes
1 | - | - | - | Yes | Yes
2 | - | - | Yes | Yes | Yes
3 | - | Yes | Yes | Yes | Yes
4 | Yes | Yes | Yes | Yes | Yes

NOTE:
This list shows the contents of the Log Output.

Log Output | Description
Trace | Detailed logs for debug
Information | Logs related to operations done on the system
Important Message | Update logs output by firmware type Installation logs by MEAP application Logs related to enabled functions by system option
Ordinary Error | Logs for ordinary errors
System Error | Logs for internal system errors

6. Press [OK] button to set the selected log level. Now the log level is successfully set.