FUNCTION

| Print out this category

FUNCTION

SORTER>FUNCTION
FIN-CON | Controller PCB RAM clear
Lv.1 | Details | To execute the RAM clear of Finisher Controller PCB to delete all the adjustment contents and counter information.
Adj/set/operate method | 1) Select the item, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | - Output the service mode setting values by P-PRINT before execution. After execution, enter necessary setting values. - The RAM data is cleared after the main power switch is turned OFF/ON.
Related service mode | COPIER> FUNCTION> MISC-P> P-PRINT