About Login Service

| Print out this category

About Login Service
The login service is started up to authenticate the user when MEAP-enabled iR device is booted up. Login service changes and install/ uninstall are carried out from the 'System Management' page. The pre-install applications and those provided on the accessory CD are as follows. Default Authentication is used as the default at the time of shipment from the factory.
CAUTION:
When the login service is set to SSO-H, Department ID management needs to be [ OFF ] before changes can be made. To use SSO-H local device authentication and Department ID management at the same time, after allocation of the department ID to the Administrator, switch the authentication method to local device authentication and then turn Department ID management ON.
To use Department ID management in domain authentication, the option image- WARE accounting manager is required.
When the setting is SSO-H, the card reader for the option controller card cannot be used.
When using SSO-H, the clock settings of the server managing the Active Directory and the MEAP device (and the PC used to log in), must be matched. If there is a time difference of greater than five minutes in the clock settings, an error will be generated when login is attempted.
When the setting is SSO-H, start up takes a little longer when compared to Default Authentication (because of the time required for object initialization).
To use the SEND function when the setting is for SSO-H, when sending email, mail addresses need to be programmed against each user. If they are not, email cannot be sent. Note, however, that when sending i-Fax, the mail addresses set in the device are used.
This device does not support SDL, conventional SSO and Security Agent. In addition these are not packaged in Administrator’s CD.