OPTION

| Print out this category

OPTION

FEEDER>OPTION
SIZE-SW | ON/OFF of mixed paper detection:AB, Inch
Lv.1 | Details | To set ON/OFF of mixed paper detection: AB configuration and Inch configuration
Use case | When enabling to mix AB and Inch configuration sizes original
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | 0 to 1 0: OFF (Mixed paper is not detected), 1: ON (Mixed paper is detected)